Beam halo data for the Digital Muon timing calibration:

HV on for (at least): a) Central Muons b) Forward Muons c) Veto Walls

ReadOut & DataLogging: [System Supervisor settings] Branches in ReadOut: 1) Central Trigger 3) Calorimeter (TailCatcher only, if possible) Branch Parameters: Calorimeter: CB-Wheel to Plug and Spacal: OFF 6) Forward Muons 11) Central Muons Logging Mode: Permanent Logging L4: Farm on Filtering & Farm Options: a) Level 2 and 4 OFF b) Full Reconstruction

Trigger: [System Supervisor settings] Trigger & Prescaling Selection: Cosmics (!!!)

General Trigger Settings: Everything OFF (Set to $00000000 !!!, verify) Trigger Mask 0: Everything OFF (Set to $00000000 !!!, verify) Trigger Mask 1: Everything OFF (Set to $00000000 !!!, verify) except: st 63 (Fwd Mu Val Any&&Veto OR Global) Trigger Mask 2: Everything OFF !!! (Set to $00000000 !!!, verify) Trigger Mask 3: Everything OFF !!! (Set to $00000000 !!!, verify) Level 2 Options: if available: Topological Trigger in

Central Trigger: [Central Trigger Mac R-301] Select Free Clock (Clock=local): Expert Menu =) Control CTC Special: HERA clock off (L4 histogram of Beam Pickup: will be flat for free clock condition)

Forward Muon Trigger: [Rack B-20 in R-307] Select Beamhalo trigger: Expert Menu =) Configuration select: Beamhalo – OK Reload everything

Do not forget to go back to Standard Conditions everywhere at the end of these special runs !